# 3D Printing Summary

|  |  |
| --- | --- |
| **Metrics** |  |
| Total Print Time (min) | 122 |
| Total Number of Components | 1 |
| Typical Total Mass (g) | 20 |
| Typical Number of Print Setups | 1 |

# 3D Printing Settings

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Print File Name** | **Qty** | **Total Print Time (hr:min)** | **Mass (g)** | **Infill (%)** | **Support** | **Layer Height/ Nozzle Diameter(mm)** | **Notes (orientation, special settings, etc.)** |
| Pull-Tab\_Tin\_Can\_Opener.stl | 1 | 2:02 | 20 | 20 | No Support | 0.2/0.4 | * Print in orientation given in STL, with flat face laying on print bed with text facing up. |

# Post-Processing

* Remove any burrs or sharp edges if applicable.

# Examples of Quality Prints

A picture containing tool, scissors, spectacles

Description automatically generated